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  Specification


Thermostatic TC-R Steam Trap
Category: Steam Trap 

Type: Thermostatic
Model: TC-R
Steam trap shall be balanced pressure type capable of operating close to saturated steam temperature. Steam trap shall be maintainable and all wetted parts shall be of 316L grade stainless steel. Steam trap shall be completely self-draining when installed in the vertical piping. Maximum operating pressure shall be 100 psig.
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